(module "Crystal_SMD_2520-4pin_2.5x2.0mm" (layer F.Cu) (tedit 5D6E9031)
  (descr "SMD Crystal SERIES SMD2520/4 http://www.newxtal.com/UploadFiles/Images/2012-11-12-09-29-09-776.pdf, 2.5x2.0mm^2 package")
  (tags "SMD SMT crystal")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.2) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value "Crystal_SMD_2520-4pin_2.5x2.0mm" (at 0 2.2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.7 -1.5) (end -1.7 -1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.7 1.5) (end 1.7 -1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.7 1.5) (end 1.7 1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.7 -1.5) (end -1.7 1.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.65 1.4) (end 1.65 1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.65 -1.4) (end -1.65 1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.25 0) (end -0.25 1) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 -0.9) (end -1.15 -1) (layer F.Fab) (width 0.1))
  (fp_line (start -1.25 0.9) (end -1.25 -0.9) (layer F.Fab) (width 0.1))
  (fp_line (start -1.15 1) (end -1.25 0.9) (layer F.Fab) (width 0.1))
  (fp_line (start 1.15 1) (end -1.15 1) (layer F.Fab) (width 0.1))
  (fp_line (start 1.25 0.9) (end 1.15 1) (layer F.Fab) (width 0.1))
  (fp_line (start 1.25 -0.9) (end 1.25 0.9) (layer F.Fab) (width 0.1))
  (fp_line (start 1.15 -1) (end 1.25 -0.9) (layer F.Fab) (width 0.1))
  (fp_line (start -1.15 -1) (end 1.15 -1) (layer F.Fab) (width 0.1))
  (fp_text user "%R" (at 0 0) (layer F.Fab)
    (effects (font (size 0.6 0.6) (thickness 0.09)))
  )
  (pad "4" smd rect (at -0.875 -0.7) (size 1.15 1) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 0.875 -0.7) (size 1.15 1) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 0.875 0.7) (size 1.15 1) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -0.875 0.7) (size 1.15 1) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.step"
    (at (xyz 0 0 0))
    (scale (xyz 0.8 0.8 1))
    (rotate (xyz 0 0 0))
  )
)
