(module "SW_SPST_3x3" (layer F.Cu) (tedit 5D5438E0)
  (descr "Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf")
  (tags "SPST Tactile Switch")
  (attr smd)
  (fp_text reference "REF**" (at 0 -2.25) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value "SW_SPST_3x3" (at 0 2.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.2 -1.6) (end -2.2 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 2.2 -1.6) (end 2.2 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.2 1.6) (end 2.2 1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.5 1.5) (end 1.5 -1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 1.5) (end -1.5 -1.5) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.5 -1.5) (end 1.5 -1.5) (layer F.SilkS) (width 0.12))
  (fp_circle (center 0 0) (end 0.9 0) (layer F.Fab) (width 0.1))
  (fp_line (start -2.2 -1.6) (end 2.2 -1.6) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 1.5) (end 1.5 1.5) (layer F.SilkS) (width 0.12))
  (fp_text user "%R" (at 0 -2.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" smd rect (at -1.8 -1.1) (size 0.7 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at 1.8 -1.1) (size 0.7 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -1.8 1.1) (size 0.7 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 1.8 1.1) (size 0.7 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.step"
    (at (xyz 0 0 0))
    (scale (xyz 0.48 0.48 0.2))
    (rotate (xyz 0 0 0))
  )
)
