(module Kailh_socket_MX (layer F.Cu) (tedit 5DD4FB17)
  (descr "MX-style keyswitch with Kailh socket mount")
  (tags MX,cherry,gateron,kailh,pg1511,socket)
  (attr smd)
  (fp_text reference REF** (at 0 -8.255) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text value Kailh_socket_MX (at 0 8.255) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -7 -6) (end -7 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -7 7) (end -6 7) (layer F.SilkS) (width 0.15))
  (fp_line (start -6 -7) (end -7 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start -7 7) (end -7 6) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 6) (end 7 7) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 -7) (end 6 -7) (layer F.SilkS) (width 0.15))
  (fp_line (start 6 7) (end 7 7) (layer F.SilkS) (width 0.15))
  (fp_line (start 7 -7) (end 7 -6) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.9 6.9) (end 6.9 6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start 6.9 -6.9) (end -6.9 -6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start 6.9 -6.9) (end 6.9 6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start -6.9 6.9) (end -6.9 -6.9) (layer Eco2.User) (width 0.15))
  (fp_line (start -7.5 -7.5) (end 7.5 -7.5) (layer F.Fab) (width 0.15))
  (fp_line (start 7.5 -7.5) (end 7.5 7.5) (layer F.Fab) (width 0.15))
  (fp_line (start 7.5 7.5) (end -7.5 7.5) (layer F.Fab) (width 0.15))
  (fp_line (start -7.5 7.5) (end -7.5 -7.5) (layer F.Fab) (width 0.15))
  (fp_arc (start -3.81 -4.445) (end -3.81 -6.985) (angle -90) (layer B.SilkS) (width 0.15))
  (fp_line (start -6.35 -1.016) (end -6.35 -0.635) (layer B.SilkS) (width 0.15))
  (fp_arc (start 0 0) (end 0 -2.54) (angle -75.96375653) (layer B.SilkS) (width 0.15))
  (fp_line (start 5.08 -3.556) (end 5.08 -2.54) (layer B.SilkS) (width 0.15))
  (fp_line (start 5.08 -2.54) (end 0 -2.54) (layer B.SilkS) (width 0.15))
  (fp_line (start -2.464162 -0.635) (end -4.191 -0.635) (layer B.SilkS) (width 0.15))
  (fp_line (start -5.969 -0.635) (end -6.35 -0.635) (layer B.SilkS) (width 0.15))
  (fp_line (start -6.35 -4.445) (end -6.35 -4.064) (layer B.SilkS) (width 0.15))
  (fp_line (start -3.81 -6.985) (end 5.08 -6.985) (layer B.SilkS) (width 0.15))
  (fp_line (start 5.08 -6.985) (end 5.08 -6.604) (layer B.SilkS) (width 0.15))
  (fp_arc (start -3.81 -4.445) (end -3.81 -6.985) (angle -90) (layer B.Fab) (width 0.12))
  (fp_arc (start 0 0) (end 0 -2.54) (angle -75.96375653) (layer B.Fab) (width 0.12))
  (fp_line (start -6.35 -0.635) (end -2.54 -0.635) (layer B.Fab) (width 0.12))
  (fp_line (start -6.35 -0.635) (end -6.35 -4.445) (layer B.Fab) (width 0.12))
  (fp_line (start -3.81 -6.985) (end 5.08 -6.985) (layer B.Fab) (width 0.12))
  (fp_line (start 5.08 -6.985) (end 5.08 -2.54) (layer B.Fab) (width 0.12))
  (fp_line (start 5.08 -2.54) (end 0 -2.54) (layer B.Fab) (width 0.12))
  (fp_line (start 5.08 -6.35) (end 7.62 -6.35) (layer B.Fab) (width 0.12))
  (fp_line (start 7.62 -6.35) (end 7.62 -3.81) (layer B.Fab) (width 0.12))
  (fp_line (start 7.62 -3.81) (end 5.08 -3.81) (layer B.Fab) (width 0.12))
  (fp_line (start -6.35 -1.27) (end -8.89 -1.27) (layer B.Fab) (width 0.12))
  (fp_line (start -8.89 -1.27) (end -8.89 -3.81) (layer B.Fab) (width 0.12))
  (fp_line (start -8.89 -3.81) (end -6.35 -3.81) (layer B.Fab) (width 0.12))
  (fp_text user %R (at -0.635 -4.445) (layer B.Fab)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user %V (at -0.635 0.635) (layer B.Fab)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (pad 1 smd rect (at 6.29 -5.08) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask))
  (pad "" np_thru_hole circle (at 2.54 -5.08) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -3.81 -2.54) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -5.08 0) (size 1.7018 1.7018) (drill 1.7018) (layers *.Cu *.Mask))
  (pad 2 smd rect (at -7.56 -2.54) (size 2.55 2.5) (layers B.Cu B.Paste B.Mask))
)
