(module "HRO-TYPE-C-31-M-12-Assembly" (layer F.Cu) (tedit 5D5436F4)
  (solder_mask_margin 0.05)
  (solder_paste_margin 0.05)
  (clearance 0.05)
  (attr smd)
  (fp_text reference "REF**" (at 0 -9.25) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value "HRO-TYPE-C-31-M-12-Assembly" (at 0 1.15) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.47 -7.3) (end 4.47 -7.3) (layer Dwgs.User) (width 0.15))
  (fp_line (start 4.47 0) (end 4.47 -7.3) (layer Dwgs.User) (width 0.15))
  (fp_line (start -4.47 0) (end -4.47 -7.3) (layer Dwgs.User) (width 0.15))
  (fp_line (start -4.47 0) (end 4.47 0) (layer Dwgs.User) (width 0.15))
  (fp_text user "%R" (at 0 -9.25) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.5 -7.5) (end -3.75 -7.5) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.5 -7.5) (end 4.5 0) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.5 0) (end -4.5 0) (layer F.CrtYd) (width 0.15))
  (fp_line (start -4.5 0) (end -4.5 -7.5) (layer F.CrtYd) (width 0.15))
  (fp_line (start -3.75 -7.5) (end -3.75 -8.5) (layer F.CrtYd) (width 0.15))
  (fp_line (start -3.75 -8.5) (end 3.75 -8.5) (layer F.CrtYd) (width 0.15))
  (fp_line (start 3.75 -8.5) (end 3.75 -7.5) (layer F.CrtYd) (width 0.15))
  (fp_line (start 4.5 -7.5) (end 3.75 -7.5) (layer F.CrtYd) (width 0.15))
  (pad "13" thru_hole oval (at 4.32 -2.6) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at -4.32 -2.6) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at 4.32 -6.78) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad "13" thru_hole oval (at -4.32 -6.78) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -2.89 -6.25) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 2.89 -6.25) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
  (pad "6" smd rect (at -0.25 -7.695) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 0.25 -7.695) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 0.75 -7.695) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -0.75 -7.695) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at 1.25 -7.695) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -1.25 -7.695) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at 1.75 -7.695) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -1.75 -7.695) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -2.45 -7.695) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at 2.45 -7.695) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -3.225 -7.695) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at 3.225 -7.695) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "/Users/danny/syncproj/kicad-libs/footprints/Keebio-Parts.pretty/3dmodels/HRO  TYPE-C-31-M-12.step"
    (offset (xyz -4.45 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
