(module ALPS_SKCM_reverse_pad (layer F.Cu) (tedit 57C14EBE)
  (descr http://deskthority.net/wiki/File:Alps_Electric_--_spec_--_5454_31.pdf)
  (tags "ALPS, keyboard switch, SKCM, SKCL")
  (fp_text reference K** (at 0 0) (layer B.SilkS)
    (effects (font (size 1.5 1.5) (thickness 0.2)) (justify mirror))
  )
  (fp_text value ALPS_SKCM (at 0 2) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9.525 9.525) (end 9.525 -9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.525 9.525) (end 9.525 9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.525 -9.525) (end 9.525 -9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.525 9.525) (end -9.525 -9.525) (layer Dwgs.User) (width 0.15))
  (fp_line (start -7.75 -6.4) (end -7.75 6.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.75 -6.4) (end 7.75 6.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.75 6.4) (end 7.75 6.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -7.75 -6.4) (end 7.75 -6.4) (layer F.SilkS) (width 0.15))
  (pad 2 thru_hole circle (at -2.5 -4) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at 2.5 -4.5) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
)
