(module ICSP-Header-ZigZag (layer F.Cu) (tedit 5C0F575F)
  (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
  (tags "Through hole socket strip THT 1x06 2.54mm single row")
  (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value ICSP (at 0 15.03) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.33 14.03) (end 1.33 14.03) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 14.03) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 1.27) (end -1.33 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 1.27) (end -1.33 14.03) (layer F.SilkS) (width 0.12))
  (fp_text user GND (at 2.032 12.7 90) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user RST (at 2.032 10.16 90) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user MOSI (at 2.032 7.62 90) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user SCK (at 2.032 5.08 90) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user VCC (at 2.032 2.54 90) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user MISO (at 2.032 0 90) (layer F.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)))
  )
  (fp_text user MOSI (at 2.032 7.62 90) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_text user SCK (at 2.032 5.08 90) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_text user MISO (at 2.032 0 90) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_text user RST (at 2.032 10.16 90) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_text user GND (at 2.032 12.7 90) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_text user VCC (at 2.032 2.54 90) (layer B.SilkS)
    (effects (font (size 0.7 0.7) (thickness 0.15)) (justify mirror))
  )
  (fp_line (start -1.27 -1.27) (end -1.27 13.97) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 13.97) (end 1.27 13.97) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 13.97) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 -1.27) (end -1.27 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start -1.33 1.27) (end -1.33 14.03) (layer B.SilkS) (width 0.12))
  (fp_line (start -1.33 14.03) (end 1.33 14.03) (layer B.SilkS) (width 0.12))
  (fp_line (start 1.33 14.03) (end 1.33 1.27) (layer B.SilkS) (width 0.12))
  (fp_line (start 1.33 1.27) (end -1.33 1.27) (layer B.SilkS) (width 0.12))
  (fp_line (start -1.33 0) (end -1.33 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.8 -1.8) (end -1.8 14.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 14.5) (end 1.8 14.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 14.5) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_text user %R (at 0 -2.33) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad 1 thru_hole rect (at -0.2286 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0.2286 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at -0.2286 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0.2286 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at -0.2286 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 0.2286 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
    (offset (xyz 0 -6.349999904632568 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 270))
  )
)
