(module YAAJ_Modules_STM32:YAAJ_BlackPill_SWD_2 (layer F.Cu) (tedit 5F81ADAB)
  (descr "BlackPill module with pin headers / sockets. SWD broken out to PCB.")
  (tags "module BlackPill Black Pill header SWD breakout")
  (fp_text reference REF** (at 8.89 -10.16) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value BlackPill (at 22.86 20.32 90) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user REF** (at 8.89 20.32 90) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user Y@@J (at 4.39238 45.2 270) (layer Dwgs.User)
    (effects (font (size 0.5 0.5) (thickness 0.1)))
  )
  (fp_line (start 3.81 -5.08) (end 3.81 -7.62) (layer F.Fab) (width 0.1))
  (fp_line (start 13.97 -5.08) (end 3.81 -5.08) (layer F.Fab) (width 0.1))
  (fp_line (start 13.97 -7.62) (end 13.97 -5.08) (layer F.Fab) (width 0.1))
  (fp_line (start 3.81 -7.62) (end 13.97 -7.62) (layer F.Fab) (width 0.1))
  (fp_line (start 4.99 43.4) (end 4.99 48.82) (layer F.Fab) (width 0.1))
  (fp_line (start 12.79 43.4) (end 4.99 43.4) (layer F.Fab) (width 0.1))
  (fp_line (start 12.79 48.82) (end 12.79 43.4) (layer F.Fab) (width 0.1))
  (fp_line (start 16.51 41.91) (end 16.51 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 19.05 41.91) (end 16.51 41.91) (layer F.Fab) (width 0.1))
  (fp_line (start 19.05 -1.27) (end 19.05 41.91) (layer F.Fab) (width 0.1))
  (fp_line (start 16.51 -1.27) (end 19.05 -1.27) (layer F.Fab) (width 0.1))
  (fp_circle (center 18.39 46.32) (end 19.89 46.32) (layer F.Fab) (width 0.1))
  (fp_circle (center -0.61 46.32) (end 0.89 46.32) (layer F.Fab) (width 0.1))
  (fp_circle (center 18.39 -5.68) (end 19.89 -5.68) (layer F.Fab) (width 0.1))
  (fp_circle (center -0.61 -5.68) (end 0.89 -5.68) (layer F.Fab) (width 0.1))
  (fp_line (start 16.45 -1.33) (end 16.45 41.97) (layer F.SilkS) (width 0.12))
  (fp_line (start 19.11 -1.33) (end 19.11 41.97) (layer F.SilkS) (width 0.12))
  (fp_line (start 16.45 -1.33) (end 19.11 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -0.635 -1.27) (end 1.27 -1.27) (layer F.Fab) (width 0.1))
  (fp_line (start 1.27 -1.27) (end 1.27 41.91) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 41.91) (end 1.27 41.91) (layer F.Fab) (width 0.1))
  (fp_line (start -1.27 41.91) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
  (fp_line (start -0.635 -1.27) (end -1.27 -0.635) (layer F.Fab) (width 0.1))
  (fp_circle (center -0.61 46.32) (end 0.9275 46.32) (layer F.SilkS) (width 0.12))
  (fp_circle (center 18.39 46.32) (end 19.9275 46.32) (layer F.SilkS) (width 0.12))
  (fp_circle (center -0.61 -5.68) (end 0.9275 -5.68) (layer F.SilkS) (width 0.12))
  (fp_circle (center 18.39 -5.68) (end 19.9275 -5.68) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.21 -8.18) (end 20.99 -8.18) (layer F.Fab) (width 0.1))
  (fp_line (start 20.99 48.82) (end 20.99 -8.18) (layer F.Fab) (width 0.1))
  (fp_line (start -3.21 -8.18) (end -3.21 48.82) (layer F.Fab) (width 0.1))
  (fp_line (start -3.302 -8.255) (end 21.082 -8.255) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.03 -7.68) (end 3.75 -7.68) (layer F.SilkS) (width 0.12))
  (fp_line (start 14.03 -5.02) (end 14.03 -7.68) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.75 -5.02) (end 14.03 -5.02) (layer F.SilkS) (width 0.12))
  (fp_line (start 3.75 -7.68) (end 3.75 -5.02) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.302 48.895) (end -3.302 -8.255) (layer F.SilkS) (width 0.12))
  (fp_line (start 21.082 -8.255) (end 21.082 48.895) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.8 -1.8) (end 1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 -1.8) (end 1.8 42.44) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 42.44) (end -1.8 42.44) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 42.44) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 19.58 -1.8) (end 19.58 42.45) (layer F.CrtYd) (width 0.05))
  (fp_line (start 15.98 -1.8) (end 19.58 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 19.58 42.44) (end 15.98 42.44) (layer F.CrtYd) (width 0.05))
  (fp_line (start 15.98 42.44) (end 15.98 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.33 1.27) (end 1.33 1.27) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 1.27) (end 1.33 41.97) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.33 41.97) (end -1.33 41.97) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 1.27) (end -1.33 41.97) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 -1.33) (end 0 -1.33) (layer F.SilkS) (width 0.12))
  (fp_line (start -1.33 -1.33) (end -1.33 0) (layer F.SilkS) (width 0.12))
  (fp_line (start 16.45 41.97) (end 19.11 41.97) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.21 48.82) (end 4.99 48.82) (layer F.Fab) (width 0.1))
  (fp_line (start 4.99 48.82) (end 4.99 49.82) (layer F.Fab) (width 0.1))
  (fp_line (start 4.99 49.82) (end 12.79 49.82) (layer F.Fab) (width 0.1))
  (fp_line (start 12.79 49.82) (end 12.79 48.82) (layer F.Fab) (width 0.1))
  (fp_line (start 12.79 48.82) (end 20.99 48.82) (layer F.Fab) (width 0.1))
  (fp_line (start -3.302 48.895) (end 4.9276 48.895) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.9276 48.895) (end 4.9276 49.8856) (layer F.SilkS) (width 0.12))
  (fp_line (start 4.9276 49.8856) (end 12.8524 49.8856) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.8524 49.8856) (end 12.8524 48.9204) (layer F.SilkS) (width 0.12))
  (fp_line (start 12.8524 48.9204) (end 21.082 48.9204) (layer F.SilkS) (width 0.12))
  (fp_line (start -3.46 -8.43) (end 21.24 -8.43) (layer F.CrtYd) (width 0.05))
  (fp_line (start 21.24 -8.43) (end 21.24 49.07) (layer F.CrtYd) (width 0.05))
  (fp_line (start 21.24 49.07) (end 13.04 49.07) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.04 49.07) (end 13.04 50.07) (layer F.CrtYd) (width 0.05))
  (fp_line (start 13.04 50.07) (end 4.74 50.07) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.74 50.07) (end 4.74 49.07) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.74 49.07) (end -3.46 49.07) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.46 49.07) (end -3.46 -8.382) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.28 -8.15) (end 14.5 -8.15) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.5 -8.15) (end 14.5 -4.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.5 -4.55) (end 3.28 -4.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.28 -4.55) (end 3.28 -8.15) (layer F.CrtYd) (width 0.05))
  (pad 38 thru_hole circle (at 5.08 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 37 thru_hole circle (at 7.62 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 36 thru_hole circle (at 10.16 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 35 thru_hole circle (at 12.7 -6.35) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 34 thru_hole circle (at 17.78 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 33 thru_hole circle (at 17.78 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 32 thru_hole circle (at 17.78 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 31 thru_hole circle (at 17.78 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 30 thru_hole circle (at 17.78 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 29 thru_hole circle (at 17.78 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 28 thru_hole circle (at 17.78 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 27 thru_hole circle (at 17.78 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 26 thru_hole circle (at 17.78 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 25 thru_hole circle (at 17.78 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 17.78 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 17.78 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 17.78 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 17.78 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 17.78 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 17.78 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 17.78 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Black_Pill/YAAJ_BlackPill_PinHeaders_B_SWD_cp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model D:/Users/admin/Documents/KiCad/Libraries/packages3d/Modules/STM32_Black_Pill/YAAJ_BlackPill_PinSockets_B_SWD_cp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
