(module "QFN-44-1EP_7x7mm_Pitch0.5mm" (layer F.Cu) (tedit 5D6E8F43)
  (descr "UK Package; 44-Lead Plastic QFN (7mm x 7mm); (see Linear Technology QFN_44_05-08-1763.pdf)")
  (tags "QFN 0.5")
  (attr smd)
  (fp_text reference "REF**" (at 0 -4.75) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "QFN-44-1EP_7x7mm_Pitch0.5mm" (at 0 4.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.5 -3.5) (end 3.5 -3.5) (layer F.Fab) (width 0.15))
  (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer F.Fab) (width 0.15))
  (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer F.Fab) (width 0.15))
  (fp_line (start -3.5 3.5) (end -3.5 -2.5) (layer F.Fab) (width 0.15))
  (fp_line (start -3.5 -2.5) (end -2.5 -3.5) (layer F.Fab) (width 0.15))
  (fp_line (start -4 -4) (end -4 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4 -4) (end 4 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4 -4) (end 4 -4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4 4) (end 4 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.625 -3.625) (end 3.625 -2.85) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.625 3.625) (end -3.625 2.85) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.625 3.625) (end 3.625 2.85) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.625 -3.625) (end -2.85 -3.625) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.625 3.625) (end -2.85 3.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.625 3.625) (end 2.85 3.625) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.625 -3.625) (end 2.85 -3.625) (layer F.SilkS) (width 0.15))
  (fp_circle (center -3.1 -3.1) (end -3.35 -3.2) (layer F.SilkS) (width 0.2))
  (pad "45" smd rect (at -1.93125 -1.93125) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at -1.93125 -0.64375) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at -1.93125 0.64375) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at -1.93125 1.93125) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at -0.64375 -1.93125) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at -0.64375 -0.64375) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at -0.64375 0.64375) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at -0.64375 1.93125) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at 0.64375 -1.93125) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at 0.64375 -0.64375) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at 0.64375 0.64375) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at 0.64375 1.93125) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at 1.93125 -1.93125) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at 1.93125 -0.64375) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at 1.93125 0.64375) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "45" smd rect (at 1.93125 1.93125) (size 1.2875 1.2875) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin_ratio -0.2))
  (pad "44" smd rect (at -2.5 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "43" smd rect (at -2 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "42" smd rect (at -1.5 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "41" smd rect (at -1 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "40" smd rect (at -0.5 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "39" smd rect (at 0 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "38" smd rect (at 0.5 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "37" smd rect (at 1 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "36" smd rect (at 1.5 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "35" smd rect (at 2 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "34" smd rect (at 2.5 -3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "33" smd rect (at 3.4 -2.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "32" smd rect (at 3.4 -2) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "31" smd rect (at 3.4 -1.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "30" smd rect (at 3.4 -1) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "29" smd rect (at 3.4 -0.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "28" smd rect (at 3.4 0) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "27" smd rect (at 3.4 0.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "26" smd rect (at 3.4 1) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd rect (at 3.4 1.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd rect (at 3.4 2) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd rect (at 3.4 2.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at 2.5 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at 2 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at 1.5 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at 1 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at 0.5 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at 0 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at -0.5 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at -1 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at -1.5 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at -2 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -2.5 3.4 90) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -3.4 2.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -3.4 2) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -3.4 1.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -3.4 1) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -3.4 0.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -3.4 0) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -3.4 -0.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -3.4 -1) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -3.4 -1.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -3.4 -2) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -3.4 -2.5) (size 0.7 0.25) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
