(module ArduinoProMicro-TopSide (layer F.Cu) (tedit 591BD5DD)
  (fp_text reference U1 (at 0 1.625) (layer F.SilkS)
    (effects (font (size 1.27 1.524) (thickness 0.2032)))
  )
  (fp_text value "Arduino Pro Micro" (at 0 0) (layer F.SilkS) hide
    (effects (font (size 1.27 1.524) (thickness 0.2032)))
  )
  (fp_text user TX0 (at -13.9 4.6 90) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user RAW (at -13.9 -4.7 90) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user RAW (at -13.9 -4.6 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user TX0 (at -13.9 4.5 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -15.24 -8.89) (end -15.24 8.89) (layer F.SilkS) (width 0.381))
  (fp_line (start -15.24 8.89) (end 15.24 8.89) (layer F.SilkS) (width 0.381))
  (fp_line (start 15.24 8.89) (end 15.24 -8.89) (layer F.SilkS) (width 0.381))
  (fp_line (start 15.24 -8.89) (end -15.24 -8.89) (layer F.SilkS) (width 0.381))
  (fp_line (start -15.24 6.35) (end -12.7 6.35) (layer F.SilkS) (width 0.381))
  (fp_line (start -12.7 6.35) (end -12.7 8.89) (layer F.SilkS) (width 0.381))
  (pad 1 thru_hole rect (at -13.97 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 2 thru_hole circle (at -11.43 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 3 thru_hole circle (at -8.89 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 4 thru_hole circle (at -6.35 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 5 thru_hole circle (at -3.81 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 6 thru_hole circle (at -1.27 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 7 thru_hole circle (at 1.27 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 8 thru_hole circle (at 3.81 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 9 thru_hole circle (at 6.35 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 10 thru_hole circle (at 8.89 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 11 thru_hole circle (at 11.43 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 13 thru_hole circle (at 13.97 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 14 thru_hole circle (at 11.43 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 15 thru_hole circle (at 8.89 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 16 thru_hole circle (at 6.35 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 17 thru_hole circle (at 3.81 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 18 thru_hole circle (at 1.27 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 19 thru_hole circle (at -1.27 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 20 thru_hole circle (at -3.81 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 21 thru_hole circle (at -6.35 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 22 thru_hole circle (at -8.89 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 23 thru_hole circle (at -11.43 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 12 thru_hole circle (at 13.97 7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (pad 24 thru_hole circle (at -13.97 -7.62) (size 1.7526 1.7526) (drill 1.0922) (layers *.Cu *.SilkS *.Mask))
  (model /Users/danny/Documents/proj/custom-keyboard/kicad-libs/3d_models/Pro_Micro.wrl
    (at (xyz 0.6 -0.35 0.05))
    (scale (xyz 0.395 0.395 0.395))
    (rotate (xyz 0 0 270))
  )
)
