(module "Header-6-Pin-ZigZag" (layer F.Cu) (tedit 5DB09E90)
  (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
  (tags "Through hole socket strip THT 1x06 2.54mm single row")
  (fp_text reference "J2" (at 0 -2.33) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "ICSP" (at 0 15.03) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.8 14.5) (end -1.8 14.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 -1.8) (end 1.8 14.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.8 -1.8) (end -1.8 14.5) (layer F.CrtYd) (width 0.05))
  (fp_line (start 1.8 -1.8) (end -1.8 -1.8) (layer F.CrtYd) (width 0.05))
  (fp_text user "%R" (at 0 -2.33) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (pad "1" thru_hole circle (at -0.2286 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "2" thru_hole oval (at 0.2286 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "3" thru_hole oval (at -0.2286 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "4" thru_hole oval (at 0.2286 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "5" thru_hole oval (at -0.2286 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "6" thru_hole oval (at 0.2286 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model "${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl"
    (offset (xyz 0 -6.349999904632568 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 270))
  )
)
