(module Kailh-PG1350-1.25u (layer F.Cu) (tedit 5D22B253)
  (fp_text reference "Kailh PG1350" (at 0 -7.14375 180) (layer Dwgs.User)
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text value Choc (at 0 -5.08 180) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.2)))
  )
  (fp_text user - (at -1.26 -3 180) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user + (at 1.27 -3 180) (layer B.SilkS)
    (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
  )
  (fp_text user - (at -1.26 -3 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user + (at 1.27 -3 180) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 6.9 6.9) (end -6.9 6.9) (layer Cmts.User) (width 0.1524))
  (fp_line (start -6.9 6.9) (end -6.9 -6.9) (layer Cmts.User) (width 0.1524))
  (fp_line (start -6.9 -6.9) (end 6.9 -6.9) (layer Cmts.User) (width 0.1524))
  (fp_line (start 6.9 -6.9) (end 6.9 6.9) (layer Cmts.User) (width 0.1524))
  (fp_line (start 9 8.5) (end -9 8.5) (layer Dwgs.User) (width 0.1524))
  (fp_line (start -9 8.5) (end -9 -8.5) (layer Dwgs.User) (width 0.1524))
  (fp_line (start -9 -8.5) (end 9 -8.5) (layer Dwgs.User) (width 0.1524))
  (fp_line (start 9 -8.5) (end 9 8.5) (layer Dwgs.User) (width 0.1524))
  (fp_line (start 7.5 7.5) (end -7.5 7.5) (layer Eco2.User) (width 0.1524))
  (fp_line (start -7.5 7.5) (end -7.5 -7.5) (layer Eco2.User) (width 0.1524))
  (fp_line (start -7.5 -7.5) (end 7.5 -7.5) (layer Eco2.User) (width 0.1524))
  (fp_line (start 7.5 -7.5) (end 7.5 7.5) (layer Eco2.User) (width 0.1524))
  (fp_line (start 11.90625 -9.525) (end 11.90625 9.525) (layer Eco1.User) (width 0.12))
  (fp_line (start -11.90625 -9.525) (end -11.90625 9.525) (layer Eco1.User) (width 0.12))
  (fp_line (start -11.90625 -9.525) (end 11.90625 -9.525) (layer Eco1.User) (width 0.12))
  (fp_line (start -11.90625 9.525) (end 11.90625 9.525) (layer Eco1.User) (width 0.12))
  (pad "" np_thru_hole circle (at 5.22 -4.2 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 0 0 180) (size 3.4 3.4) (drill 3.4) (layers *.Cu *.Mask))
  (pad 4 thru_hole rect (at -1.27 -4.8 180) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 1.27 -4.8 180) (size 1.905 1.905) (drill 0.9906) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 5.9 180) (size 2 2) (drill 1.2) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -5 3.8 41.9) (size 2 2) (drill 1.2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -5.5 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 5.5 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (model /Users/danny/Documents/proj/custom-keyboard/kicad-libs/3d_models/mx-switch.wrl
    (offset (xyz 7.4675998878479 7.4675998878479 5.943599910736085))
    (scale (xyz 0.4 0.4 0.4))
    (rotate (xyz 270 0 180))
  )
  (model /Users/danny/Documents/proj/custom-keyboard/kicad-libs/3d_models/SA-R3-1u.wrl
    (offset (xyz 0 0 11.93799982070923))
    (scale (xyz 0.394 0.394 0.394))
    (rotate (xyz 270 0 0))
  )
)
