(module 00Keyboard:SW_ALPS_SSAA (layer F.Cu)
  (fp_text reference SW_ALPS_SSAA (at -0.05 0.05) (layer F.SilkS) hide
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_text value SW** (at 0 4.1) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.15)))
  )
  (fp_line (start 5.2 -3) (end 5.2 3) (layer Dwgs.User) (width 0.16))
  (fp_line (start 5.2 3) (end -5.2 3) (layer Dwgs.User) (width 0.16))
  (fp_line (start -5.2 3) (end -5.2 -3) (layer Dwgs.User) (width 0.16))
  (fp_line (start -5.2 -3) (end 5.2 -3) (layer Dwgs.User) (width 0.16))
  (fp_line (start 4.75 -5) (end -2.25 -5) (layer Dwgs.User) (width 0.16))
  (fp_line (start 2.5 -5.6) (end 4.75 -5.6) (layer Dwgs.User) (width 0.16))
  (fp_line (start 4.75 -5.6) (end 4.75 -5) (layer Dwgs.User) (width 0.16))
  (fp_line (start -2.25 -5) (end -2.25 -5.6) (layer Dwgs.User) (width 0.16))
  (fp_line (start -2.25 -5.6) (end 0 -5.6) (layer Dwgs.User) (width 0.16))
  (fp_line (start 0 -6.95) (end 0 -5.6) (layer Dwgs.User) (width 0.16))
  (fp_line (start 0 -7) (end 2.5 -7) (layer Dwgs.User) (width 0.16))
  (fp_line (start 2.5 -7) (end 2.5 -5.6) (layer Dwgs.User) (width 0.16))
  (pad 5 thru_hole circle (at -2 -1.25) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at 2 -1.25) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 0 -1.25) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at 0 1.25) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 2 1.25) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -2 1.25) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole circle (at 5 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole circle (at -5 0) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
)
