(module "MX_FMask-with-cutout" (layer F.Cu) (tedit 5DDAB8EA)
  (fp_text reference "REF**" (at 0.25 10.05) (layer Eco2.User) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "MX_FMask-with-cutout" (at 0 -15.24) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 9.5 -9.5) (end 9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 9.5) (end -9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.5 9.5) (end -9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.5 -9.5) (end 9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 7 -7) (end -7 -7) (layer Edge.Cuts) (width 0.15))
  (fp_line (start -7 -7) (end -7 7) (layer Edge.Cuts) (width 0.15))
  (fp_line (start -7 7) (end 7 7) (layer Edge.Cuts) (width 0.15))
  (fp_line (start 7 7) (end 7 -7) (layer Edge.Cuts) (width 0.15))
  (pad "1" smd roundrect (at 0 0 180) (size 16 16) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.063))
  (pad "1" smd roundrect (at 0 0 180) (size 16 16) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.063))
)
