(module MX_Stabilizer_Cutout (layer F.Cu) (tedit 59615D2E)
  (fp_text reference REF** (at 0.25 10.05) (layer Eco2.User) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MX-Alps_Switch_Cutout (at 0 -15.24) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -9.5 -9.5) (end 9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.5 9.5) (end -9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 9.5) (end -9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 -9.5) (end 9.5 9.5) (layer Dwgs.User) (width 0.15))
  (pad "" np_thru_hole oval (at 0 7.7724) (size 3.048 0.3048) (drill oval 3.048 0.3048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 0 -5.5372) (size 6.6548 0.3048) (drill oval 6.6548 0.3048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -3.175 0.4572) (size 0.3048 12.2936) (drill oval 0.3048 12.2936) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 0 6.4516) (size 6.6548 0.3048) (drill oval 6.6548 0.3048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 3.175 0.4572) (size 0.3048 12.2936) (drill oval 0.3048 12.2936) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -4.0386 -0.889) (size 0.3048 2.794) (drill oval 0.3048 2.794) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -1.3716 7.112) (size 0.3048 1.4732) (drill oval 0.3048 1.4732) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -3.6068 -2.1336) (size 1.1684 0.3048) (drill oval 1.1684 0.3048) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at 1.3716 7.112) (size 0.3048 1.4732) (drill oval 0.3048 1.4732) (layers *.Cu *.Mask))
  (pad "" np_thru_hole oval (at -3.6068 0.3556) (size 1.1684 0.3048) (drill oval 1.1684 0.3048) (layers *.Cu *.Mask))
)
