(module MX-Alps_Switch_Cutout (layer F.Cu) (tedit 5BEEFD84)
  (fp_text reference REF** (at 0.25 10.05) (layer Eco2.User) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value MX-Alps_Switch_Cutout (at 0 -15.24) (layer F.Fab) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -9.5 -9.5) (end 9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -9.5 9.5) (end -9.5 -9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 9.5) (end -9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start 9.5 -9.5) (end 9.5 9.5) (layer Dwgs.User) (width 0.15))
  (fp_line (start -6.85 -6.25) (end -6.85 -7) (layer Edge.Cuts) (width 0.12))
  (fp_line (start -6.85 -7) (end 6.85 -7) (layer Edge.Cuts) (width 0.12))
  (fp_line (start 6.85 -7) (end 6.85 -6.25) (layer Edge.Cuts) (width 0.12))
  (fp_line (start 6.85 -6.25) (end 7.8 -6.25) (layer Edge.Cuts) (width 0.12))
  (fp_line (start 7.8 -6.25) (end 7.8 6.25) (layer Edge.Cuts) (width 0.12))
  (fp_line (start 7.8 6.25) (end 6.85 6.25) (layer Edge.Cuts) (width 0.12))
  (fp_line (start 6.85 6.25) (end 6.85 7) (layer Edge.Cuts) (width 0.12))
  (fp_line (start 6.85 7) (end -6.85 7) (layer Edge.Cuts) (width 0.12))
  (fp_line (start -6.85 7) (end -6.85 6.25) (layer Edge.Cuts) (width 0.12))
  (fp_line (start -6.85 6.25) (end -7.8 6.25) (layer Edge.Cuts) (width 0.12))
  (fp_line (start -7.8 6.25) (end -7.8 -6.25) (layer Edge.Cuts) (width 0.12))
  (fp_line (start -7.8 -6.25) (end -6.85 -6.25) (layer Edge.Cuts) (width 0.12))
  (pad 1 smd roundrect (at 0 0 180) (size 17.4 15.8) (layers F.Mask F.Cu) (roundrect_rratio 0.063))
  (pad 1 smd roundrect (at 0 0 180) (size 17.4 15.8) (layers B.Mask B.Cu) (roundrect_rratio 0.063))
)
